--------------------------------------------------------------------------------
Library :MurataDynamicModel_C
Conponent name : GCE18_D
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GCE18_D

PartNumber | tmpr | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GCE188R71H102KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H102MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A102KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A102MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H122KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H122MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A122KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A122MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H152KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1500[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H152MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1500[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A152KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1500[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A152MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1500[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H182KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H182MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1800[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A182KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A182MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1800[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H222KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H222MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 2200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A222KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A222MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 2200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H272KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 2700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H272MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 2700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A272KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 2700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A272MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 2700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H332KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 3300[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H332MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 3300[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A332KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 3300[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A332MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 3300[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H392KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 3900[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H392MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 3900[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A392KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 3900[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A392MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 3900[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H472KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H472MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 4700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A472KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A472MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 4700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H562KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 5600[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H562MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 5600[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A562KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 5600[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A562MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 5600[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H682KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 6800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H682MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 6800[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A682KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 6800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A682MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 6800[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H822KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 8200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H822MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 8200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A822KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 8200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A822MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 8200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H103KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H103MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A103KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A103MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H123KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 12000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H123MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 12000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A123KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 12000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A123MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 12000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H153KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 15000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H153MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 15000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A153KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 15000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A153MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 15000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H183KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 18000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H183MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 18000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A183KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 18000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A183MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 18000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H223KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71H223MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 22000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A223KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R72A223MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 22000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71E273KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 27000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71E273MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 27000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71E333KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 33000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71E333MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 33000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71E393KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 39000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71E393MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 39000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71E473KA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 47000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCE188R71E473MA01 | 25 | Specially designed product to reduce shorts & resin electrode product | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 47000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]